#MicroXplorer Configuration settings - do not modify
CAD.formats=
CAD.pinconfig=
CAD.provider=
DMA2D.ColorMode=DMA2D_OUTPUT_ARGB8888
DMA2D.IPParameters=ColorMode
Dma.I2C1_RX.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.I2C1_RX.0.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.I2C1_RX.0.Instance=DMA1_Stream0
Dma.I2C1_RX.0.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.I2C1_RX.0.MemInc=DMA_MINC_ENABLE
Dma.I2C1_RX.0.Mode=DMA_NORMAL
Dma.I2C1_RX.0.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.I2C1_RX.0.PeriphInc=DMA_PINC_DISABLE
Dma.I2C1_RX.0.Priority=DMA_PRIORITY_LOW
Dma.I2C1_RX.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.I2C1_TX.1.Direction=DMA_MEMORY_TO_PERIPH
Dma.I2C1_TX.1.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.I2C1_TX.1.Instance=DMA1_Stream6
Dma.I2C1_TX.1.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.I2C1_TX.1.MemInc=DMA_MINC_ENABLE
Dma.I2C1_TX.1.Mode=DMA_NORMAL
Dma.I2C1_TX.1.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.I2C1_TX.1.PeriphInc=DMA_PINC_DISABLE
Dma.I2C1_TX.1.Priority=DMA_PRIORITY_LOW
Dma.I2C1_TX.1.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.Request0=I2C1_RX
Dma.Request1=I2C1_TX
Dma.Request2=USART1_RX
Dma.Request3=USART1_TX
Dma.RequestsNb=4
Dma.USART1_RX.2.Direction=DMA_PERIPH_TO_MEMORY
Dma.USART1_RX.2.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART1_RX.2.Instance=DMA2_Stream2
Dma.USART1_RX.2.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART1_RX.2.MemInc=DMA_MINC_ENABLE
Dma.USART1_RX.2.Mode=DMA_NORMAL
Dma.USART1_RX.2.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART1_RX.2.PeriphInc=DMA_PINC_DISABLE
Dma.USART1_RX.2.Priority=DMA_PRIORITY_LOW
Dma.USART1_RX.2.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
Dma.USART1_TX.3.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART1_TX.3.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.USART1_TX.3.Instance=DMA2_Stream7
Dma.USART1_TX.3.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART1_TX.3.MemInc=DMA_MINC_ENABLE
Dma.USART1_TX.3.Mode=DMA_NORMAL
Dma.USART1_TX.3.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART1_TX.3.PeriphInc=DMA_PINC_DISABLE
Dma.USART1_TX.3.Priority=DMA_PRIORITY_LOW
Dma.USART1_TX.3.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode
FATFS.IPParameters=_CODE_PAGE,_USE_LFN,_MAX_SS,_FS_TINY
FATFS._CODE_PAGE=936
FATFS._FS_TINY=1
FATFS._MAX_SS=4096
FATFS._USE_LFN=2
FMC.CASLatency1=FMC_SDRAM_CAS_LATENCY_3
FMC.ExitSelfRefreshDelay1=7
FMC.IPParameters=CASLatency1,SDClockPeriod1,ReadPipeDelay1,LoadToActiveDelay1,ExitSelfRefreshDelay1,SelfRefreshTime1,RowCycleDelay1,WriteRecoveryTime1,RPDelay1,RCDDelay1
FMC.LoadToActiveDelay1=2
FMC.RCDDelay1=2
FMC.RPDelay1=2
FMC.ReadPipeDelay1=FMC_SDRAM_RPIPE_DELAY_1
FMC.RowCycleDelay1=6
FMC.SDClockPeriod1=FMC_SDRAM_CLOCK_PERIOD_2
FMC.SelfRefreshTime1=4
FMC.WriteRecoveryTime1=3
FREERTOS.FootprintOK=true
FREERTOS.IPParameters=Tasks01,FootprintOK,configUSE_IDLE_HOOK,configUSE_TICK_HOOK,configCHECK_FOR_STACK_OVERFLOW
FREERTOS.Tasks01=defaultTask,24,2048,StartDefaultTask,As weak,NULL,Dynamic,NULL,NULL
FREERTOS.configCHECK_FOR_STACK_OVERFLOW=2
FREERTOS.configUSE_IDLE_HOOK=1
FREERTOS.configUSE_TICK_HOOK=1
File.Version=6
GPIO.groupedBy=Group By Peripherals
KeepUserPlacement=false
LTDC.ActiveH=272
LTDC.ActiveW=480
LTDC.FBStartAdress_L0=LCD_BANK_ADDRESS
LTDC.FBStartAdress_L1=LCD_BANK_ADDRESS+LCD_PIX_WIDTH*LCD_PIX_HEIGHT*LCD_PIX_SIZE
LTDC.IPParameters=WindowY0_L0,WindowY1_L0,ActiveW,ActiveH,WindowX1_L0,WindowX1_L1,WindowY1_L1,VFP,ImageWidth_L0,ImageHeight_L0,FBStartAdress_L0,ImageWidth_L1,ImageHeight_L1,FBStartAdress_L1
LTDC.ImageHeight_L0=LCD_PIX_HEIGHT
LTDC.ImageHeight_L1=LCD_PIX_HEIGHT
LTDC.ImageWidth_L0=LCD_PIX_WIDTH
LTDC.ImageWidth_L1=LCD_PIX_WIDTH
LTDC.VFP=4
LTDC.WindowX1_L0=480
LTDC.WindowX1_L1=480
LTDC.WindowY0_L0=0
LTDC.WindowY1_L0=272
LTDC.WindowY1_L1=272
Mcu.CPN=STM32F429IGT6
Mcu.Family=STM32F4
Mcu.IP0=DMA
Mcu.IP1=DMA2D
Mcu.IP10=SYS
Mcu.IP11=TIM7
Mcu.IP12=USART1
Mcu.IP13=USB_DEVICE
Mcu.IP14=USB_OTG_HS
Mcu.IP2=FATFS
Mcu.IP3=FMC
Mcu.IP4=FREERTOS
Mcu.IP5=I2C1
Mcu.IP6=LTDC
Mcu.IP7=NVIC
Mcu.IP8=RCC
Mcu.IP9=SPI5
Mcu.IPNb=15
Mcu.Name=STM32F429I(E-G)Tx
Mcu.Package=LQFP176
Mcu.Pin0=PE4
Mcu.Pin1=PE5
Mcu.Pin10=PF4
Mcu.Pin11=PF5
Mcu.Pin12=PF6
Mcu.Pin13=PF7
Mcu.Pin14=PF8
Mcu.Pin15=PF9
Mcu.Pin16=PF10
Mcu.Pin17=PH0/OSC_IN
Mcu.Pin18=PH1/OSC_OUT
Mcu.Pin19=PC0
Mcu.Pin2=PE6
Mcu.Pin20=PA0/WKUP
Mcu.Pin21=PH2
Mcu.Pin22=PH3
Mcu.Pin23=PA3
Mcu.Pin24=PB0
Mcu.Pin25=PB1
Mcu.Pin26=PF11
Mcu.Pin27=PF12
Mcu.Pin28=PF13
Mcu.Pin29=PF14
Mcu.Pin3=PC13
Mcu.Pin30=PF15
Mcu.Pin31=PG0
Mcu.Pin32=PG1
Mcu.Pin33=PE7
Mcu.Pin34=PE8
Mcu.Pin35=PE9
Mcu.Pin36=PE10
Mcu.Pin37=PE11
Mcu.Pin38=PE12
Mcu.Pin39=PE13
Mcu.Pin4=PI9
Mcu.Pin40=PE14
Mcu.Pin41=PE15
Mcu.Pin42=PH6
Mcu.Pin43=PH7
Mcu.Pin44=PH8
Mcu.Pin45=PH10
Mcu.Pin46=PB14
Mcu.Pin47=PB15
Mcu.Pin48=PD8
Mcu.Pin49=PD9
Mcu.Pin5=PI10
Mcu.Pin50=PD10
Mcu.Pin51=PD14
Mcu.Pin52=PD15
Mcu.Pin53=PG2
Mcu.Pin54=PG4
Mcu.Pin55=PG5
Mcu.Pin56=PG6
Mcu.Pin57=PG7
Mcu.Pin58=PG8
Mcu.Pin59=PC7
Mcu.Pin6=PF0
Mcu.Pin60=PA9
Mcu.Pin61=PA10
Mcu.Pin62=PA11
Mcu.Pin63=PA12
Mcu.Pin64=PA13
Mcu.Pin65=PH13
Mcu.Pin66=PH15
Mcu.Pin67=PI0
Mcu.Pin68=PI2
Mcu.Pin69=PA14
Mcu.Pin7=PF1
Mcu.Pin70=PD0
Mcu.Pin71=PD1
Mcu.Pin72=PD4
Mcu.Pin73=PD6
Mcu.Pin74=PD7
Mcu.Pin75=PG9
Mcu.Pin76=PG10
Mcu.Pin77=PG11
Mcu.Pin78=PG12
Mcu.Pin79=PG15
Mcu.Pin8=PF2
Mcu.Pin80=PB6
Mcu.Pin81=PB7
Mcu.Pin82=PB8
Mcu.Pin83=PB9
Mcu.Pin84=PE0
Mcu.Pin85=PE1
Mcu.Pin86=PI4
Mcu.Pin87=VP_DMA2D_VS_DMA2D
Mcu.Pin88=VP_FATFS_VS_Generic
Mcu.Pin89=VP_FREERTOS_VS_CMSIS_V2
Mcu.Pin9=PF3
Mcu.Pin90=VP_SYS_VS_tim6
Mcu.Pin91=VP_TIM7_VS_ClockSourceINT
Mcu.Pin92=VP_USB_DEVICE_VS_USB_DEVICE_MSC_HS
Mcu.PinsNb=93
Mcu.ThirdPartyNb=0
Mcu.UserConstants=LCD_BANK_ADDRESS,0xD0000000;LCD_PIX_WIDTH,480;LCD_PIX_HEIGHT,272;LCD_PIX_SIZE,4
Mcu.UserName=STM32F429IGTx
MxCube.Version=6.9.2
MxDb.Version=DB.6.0.92
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.DMA1_Stream0_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC.DMA1_Stream6_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC.DMA2D_IRQn=true\:5\:0\:false\:false\:false\:true\:true\:true\:true
NVIC.DMA2_Stream2_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC.DMA2_Stream7_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.I2C1_ER_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.I2C1_EV_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.LTDC_IRQn=true\:5\:0\:false\:false\:false\:true\:true\:true\:true
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.OTG_HS_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true\:true
NVIC.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=true
NVIC.SavedSvcallIrqHandlerGenerated=true
NVIC.SavedSystickIrqHandlerGenerated=true
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:true\:false
NVIC.TIM6_DAC_IRQn=true\:15\:0\:false\:false\:true\:false\:false\:true\:true
NVIC.TIM7_IRQn=true\:5\:0\:false\:false\:false\:true\:true\:true\:true
NVIC.TimeBase=TIM6_DAC_IRQn
NVIC.TimeBaseIP=TIM6
NVIC.USART1_IRQn=true\:5\:0\:false\:false\:false\:true\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
PA0/WKUP.GPIOParameters=GPIO_Label
PA0/WKUP.GPIO_Label=KEY1
PA0/WKUP.Locked=true
PA0/WKUP.Signal=GPXTI0
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA11.GPIOParameters=GPIO_Speed,GPIO_PuPd
PA11.GPIO_PuPd=GPIO_PULLUP
PA11.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA11.Mode=RGB888
PA11.Signal=LTDC_R4
PA12.GPIOParameters=GPIO_Speed,GPIO_PuPd
PA12.GPIO_PuPd=GPIO_PULLUP
PA12.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA12.Locked=true
PA12.Mode=RGB888
PA12.Signal=LTDC_R5
PA13.Mode=Serial_Wire
PA13.Signal=SYS_JTMS-SWDIO
PA14.Mode=Serial_Wire
PA14.Signal=SYS_JTCK-SWCLK
PA3.GPIOParameters=GPIO_Speed,GPIO_PuPd
PA3.GPIO_PuPd=GPIO_PULLUP
PA3.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA3.Mode=RGB888
PA3.Signal=LTDC_B5
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB0.GPIOParameters=GPIO_Speed,GPIO_PuPd
PB0.GPIO_PuPd=GPIO_PULLUP
PB0.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PB0.Mode=RGB888
PB0.Signal=LTDC_R3
PB1.GPIOParameters=GPIO_Speed,GPIO_PuPd
PB1.GPIO_PuPd=GPIO_PULLUP
PB1.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PB1.Mode=RGB888
PB1.Signal=LTDC_R6
PB14.Mode=Device_Only_FS
PB14.Signal=USB_OTG_HS_DM
PB15.Mode=Device_Only_FS
PB15.Signal=USB_OTG_HS_DP
PB6.Mode=I2C
PB6.Signal=I2C1_SCL
PB7.Mode=I2C
PB7.Signal=I2C1_SDA
PB8.GPIOParameters=GPIO_Speed,GPIO_PuPd
PB8.GPIO_PuPd=GPIO_PULLUP
PB8.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PB8.Mode=RGB888
PB8.Signal=LTDC_B6
PB9.GPIOParameters=GPIO_Speed,GPIO_PuPd
PB9.GPIO_PuPd=GPIO_PULLUP
PB9.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PB9.Mode=RGB888
PB9.Signal=LTDC_B7
PC0.Signal=FMC_SDNWE
PC13.GPIOParameters=GPIO_Label
PC13.GPIO_Label=KEY2
PC13.Locked=true
PC13.Signal=GPXTI13
PC7.GPIOParameters=GPIO_Speed,GPIO_PuPd
PC7.GPIO_PuPd=GPIO_PULLUP
PC7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PC7.Mode=RGB888
PC7.Signal=LTDC_G6
PD0.Signal=FMC_D2_DA2
PD1.Signal=FMC_D3_DA3
PD10.Signal=FMC_D15_DA15
PD14.Signal=FMC_D0_DA0
PD15.Signal=FMC_D1_DA1
PD4.GPIOParameters=GPIO_Label
PD4.GPIO_Label=LTDC_DISP
PD4.Locked=true
PD4.Signal=GPIO_Output
PD6.GPIOParameters=GPIO_Speed,GPIO_PuPd
PD6.GPIO_PuPd=GPIO_PULLUP
PD6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PD6.Locked=true
PD6.Mode=RGB888
PD6.Signal=LTDC_B2
PD7.GPIOParameters=GPIO_Label
PD7.GPIO_Label=LTDC_BL
PD7.Locked=true
PD7.Signal=GPIO_Output
PD8.Signal=FMC_D13_DA13
PD9.Signal=FMC_D14_DA14
PE0.Signal=FMC_NBL0
PE1.Signal=FMC_NBL1
PE10.Signal=FMC_D7_DA7
PE11.Signal=FMC_D8_DA8
PE12.Signal=FMC_D9_DA9
PE13.Signal=FMC_D10_DA10
PE14.Signal=FMC_D11_DA11
PE15.Signal=FMC_D12_DA12
PE4.GPIOParameters=GPIO_Speed,GPIO_PuPd
PE4.GPIO_PuPd=GPIO_PULLUP
PE4.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PE4.Locked=true
PE4.Mode=RGB888
PE4.Signal=LTDC_B0
PE5.GPIOParameters=GPIO_Speed,GPIO_PuPd
PE5.GPIO_PuPd=GPIO_PULLUP
PE5.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PE5.Locked=true
PE5.Mode=RGB888
PE5.Signal=LTDC_G0
PE6.GPIOParameters=GPIO_Speed,GPIO_PuPd
PE6.GPIO_PuPd=GPIO_PULLUP
PE6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PE6.Locked=true
PE6.Mode=RGB888
PE6.Signal=LTDC_G1
PE7.Signal=FMC_D4_DA4
PE8.Signal=FMC_D5_DA5
PE9.Signal=FMC_D6_DA6
PF0.Signal=FMC_A0
PF1.Signal=FMC_A1
PF10.GPIOParameters=GPIO_Speed,GPIO_PuPd
PF10.GPIO_PuPd=GPIO_PULLUP
PF10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PF10.Mode=RGB888
PF10.Signal=LTDC_DE
PF11.Signal=FMC_SDNRAS
PF12.Signal=FMC_A6
PF13.Signal=FMC_A7
PF14.Signal=FMC_A8
PF15.Signal=FMC_A9
PF2.Signal=FMC_A2
PF3.Signal=FMC_A3
PF4.Signal=FMC_A4
PF5.Signal=FMC_A5
PF6.GPIOParameters=GPIO_Label
PF6.GPIO_Label=SPI5_CS
PF6.Locked=true
PF6.Signal=GPIO_Output
PF7.Mode=Full_Duplex_Master
PF7.Signal=SPI5_SCK
PF8.Mode=Full_Duplex_Master
PF8.Signal=SPI5_MISO
PF9.Mode=Full_Duplex_Master
PF9.Signal=SPI5_MOSI
PG0.Signal=FMC_A10
PG1.Signal=FMC_A11
PG10.GPIOParameters=GPIO_Speed,GPIO_PuPd
PG10.GPIO_PuPd=GPIO_PULLUP
PG10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG10.Locked=true
PG10.Mode=RGB888
PG10.Signal=LTDC_G3
PG11.GPIOParameters=GPIO_Speed,GPIO_PuPd
PG11.GPIO_PuPd=GPIO_PULLUP
PG11.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG11.Mode=RGB888
PG11.Signal=LTDC_B3
PG12.GPIOParameters=GPIO_Speed,GPIO_PuPd
PG12.GPIO_PuPd=GPIO_PULLUP
PG12.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG12.Locked=true
PG12.Mode=RGB888
PG12.Signal=LTDC_B1
PG15.Signal=FMC_SDNCAS
PG2.Signal=FMC_A12
PG4.Signal=FMC_A14_BA0
PG5.Signal=FMC_A15_BA1
PG6.GPIOParameters=GPIO_Speed,GPIO_PuPd
PG6.GPIO_PuPd=GPIO_PULLUP
PG6.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG6.Mode=RGB888
PG6.Signal=LTDC_R7
PG7.GPIOParameters=GPIO_Speed,GPIO_PuPd
PG7.GPIO_PuPd=GPIO_PULLUP
PG7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG7.Mode=RGB888
PG7.Signal=LTDC_CLK
PG8.Signal=FMC_SDCLK
PG9.Mode=NandChipSelect3_2
PG9.Signal=FMC_NCE3
PH0/OSC_IN.Mode=HSE-External-Oscillator
PH0/OSC_IN.Signal=RCC_OSC_IN
PH1/OSC_OUT.Mode=HSE-External-Oscillator
PH1/OSC_OUT.Signal=RCC_OSC_OUT
PH10.GPIOParameters=GPIO_Label
PH10.GPIO_Label=LED1
PH10.Locked=true
PH10.Signal=GPIO_Output
PH13.GPIOParameters=GPIO_Speed,GPIO_PuPd
PH13.GPIO_PuPd=GPIO_PULLUP
PH13.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH13.Locked=true
PH13.Mode=RGB888
PH13.Signal=LTDC_G2
PH15.GPIOParameters=GPIO_Speed,GPIO_PuPd
PH15.GPIO_PuPd=GPIO_PULLUP
PH15.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH15.Locked=true
PH15.Mode=RGB888
PH15.Signal=LTDC_G4
PH2.GPIOParameters=GPIO_Speed,GPIO_PuPd
PH2.GPIO_PuPd=GPIO_PULLUP
PH2.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH2.Locked=true
PH2.Mode=RGB888
PH2.Signal=LTDC_R0
PH3.GPIOParameters=GPIO_Speed,GPIO_PuPd
PH3.GPIO_PuPd=GPIO_PULLUP
PH3.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH3.Locked=true
PH3.Mode=RGB888
PH3.Signal=LTDC_R1
PH6.Mode=SdramChipSelect2_1
PH6.Signal=FMC_SDNE1
PH7.Mode=SdramChipSelect2_1
PH7.Signal=FMC_SDCKE1
PH8.GPIOParameters=GPIO_Speed,GPIO_PuPd
PH8.GPIO_PuPd=GPIO_PULLUP
PH8.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PH8.Locked=true
PH8.Mode=RGB888
PH8.Signal=LTDC_R2
PI0.GPIOParameters=GPIO_Speed,GPIO_PuPd
PI0.GPIO_PuPd=GPIO_PULLUP
PI0.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI0.Locked=true
PI0.Mode=RGB888
PI0.Signal=LTDC_G5
PI10.GPIOParameters=GPIO_Speed
PI10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI10.Mode=RGB888
PI10.Signal=LTDC_HSYNC
PI2.GPIOParameters=GPIO_Speed,GPIO_PuPd
PI2.GPIO_PuPd=GPIO_PULLUP
PI2.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI2.Mode=RGB888
PI2.Signal=LTDC_G7
PI4.GPIOParameters=GPIO_Speed
PI4.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI4.Locked=true
PI4.Mode=RGB888
PI4.Signal=LTDC_B4
PI9.GPIOParameters=GPIO_Speed
PI9.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PI9.Mode=RGB888
PI9.Signal=LTDC_VSYNC
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=true
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F429IGTx
ProjectManager.FirmwarePackage=STM32Cube FW_F4 V1.27.1
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x1000
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=0
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=429IGT6.ioc
ProjectManager.ProjectName=429IGT6
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x1500
ProjectManager.TargetToolchain=Makefile
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=false
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false,2-MX_GPIO_Init-GPIO-false-HAL-true,3-MX_DMA_Init-DMA-false-HAL-true,4-MX_I2C1_Init-I2C1-false-HAL-true,5-MX_TIM7_Init-TIM7-false-HAL-true,6-MX_USART1_UART_Init-USART1-false-HAL-true,7-MX_SPI5_Init-SPI5-false-HAL-true,8-MX_FATFS_Init-FATFS-false-HAL-false,9-MX_USB_DEVICE_Init-USB_DEVICE-false-HAL-false,10-MX_FMC_Init-FMC-false-HAL-true,11-MX_DMA2D_Init-DMA2D-false-HAL-true,12-MX_LTDC_Init-LTDC-false-HAL-true
RCC.48MHZClocksFreq_Value=48000000
RCC.AHBFreq_Value=168000000
RCC.APB1CLKDivider=RCC_HCLK_DIV4
RCC.APB1Freq_Value=42000000
RCC.APB1TimFreq_Value=84000000
RCC.APB2CLKDivider=RCC_HCLK_DIV2
RCC.APB2Freq_Value=84000000
RCC.APB2TimFreq_Value=168000000
RCC.CortexFreq_Value=168000000
RCC.EthernetFreq_Value=168000000
RCC.FCLKCortexFreq_Value=168000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=168000000
RCC.HSE_VALUE=25000000
RCC.HSI_VALUE=16000000
RCC.I2SClocksFreq_Value=96000000
RCC.IPParameters=48MHZClocksFreq_Value,AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,CortexFreq_Value,EthernetFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI_VALUE,I2SClocksFreq_Value,LCDTFTFreq_Value,LSE_VALUE,LSI_VALUE,MCO2PinFreq_Value,PLLCLKFreq_Value,PLLM,PLLN,PLLQ,PLLQCLKFreq_Value,PLLSAIDivR,PLLSAIN,PLLSAIR,RTCFreq_Value,RTCHSEDivFreq_Value,SAI_AClocksFreq_Value,SAI_BClocksFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,VCOI2SOutputFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAIOutputFreq_Value,VCOSAIOutputFreq_ValueQ,VCOSAIOutputFreq_ValueR,VcooutputI2S,VcooutputI2SQ
RCC.LCDTFTFreq_Value=9600000
RCC.LSE_VALUE=32768
RCC.LSI_VALUE=32000
RCC.MCO2PinFreq_Value=168000000
RCC.PLLCLKFreq_Value=168000000
RCC.PLLM=25
RCC.PLLN=336
RCC.PLLQ=7
RCC.PLLQCLKFreq_Value=48000000
RCC.PLLSAIDivR=RCC_PLLSAIDIVR_4
RCC.PLLSAIN=192
RCC.PLLSAIR=5
RCC.RTCFreq_Value=32000
RCC.RTCHSEDivFreq_Value=12500000
RCC.SAI_AClocksFreq_Value=48000000
RCC.SAI_BClocksFreq_Value=48000000
RCC.SYSCLKFreq_VALUE=168000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.VCOI2SOutputFreq_Value=192000000
RCC.VCOInputFreq_Value=1000000
RCC.VCOOutputFreq_Value=336000000
RCC.VCOSAIOutputFreq_Value=192000000
RCC.VCOSAIOutputFreq_ValueQ=48000000
RCC.VCOSAIOutputFreq_ValueR=38400000
RCC.VcooutputI2S=96000000
RCC.VcooutputI2SQ=96000000
SH.FMC_A0.0=FMC_A0,13b-sda1
SH.FMC_A0.ConfNb=1
SH.FMC_A1.0=FMC_A1,13b-sda1
SH.FMC_A1.ConfNb=1
SH.FMC_A10.0=FMC_A10,13b-sda1
SH.FMC_A10.ConfNb=1
SH.FMC_A11.0=FMC_A11,13b-sda1
SH.FMC_A11.ConfNb=1
SH.FMC_A12.0=FMC_A12,13b-sda1
SH.FMC_A12.ConfNb=1
SH.FMC_A14_BA0.0=FMC_BA0,FourSdramBanks1
SH.FMC_A14_BA0.ConfNb=1
SH.FMC_A15_BA1.0=FMC_BA1,FourSdramBanks1
SH.FMC_A15_BA1.ConfNb=1
SH.FMC_A2.0=FMC_A2,13b-sda1
SH.FMC_A2.ConfNb=1
SH.FMC_A3.0=FMC_A3,13b-sda1
SH.FMC_A3.ConfNb=1
SH.FMC_A4.0=FMC_A4,13b-sda1
SH.FMC_A4.ConfNb=1
SH.FMC_A5.0=FMC_A5,13b-sda1
SH.FMC_A5.ConfNb=1
SH.FMC_A6.0=FMC_A6,13b-sda1
SH.FMC_A6.ConfNb=1
SH.FMC_A7.0=FMC_A7,13b-sda1
SH.FMC_A7.ConfNb=1
SH.FMC_A8.0=FMC_A8,13b-sda1
SH.FMC_A8.ConfNb=1
SH.FMC_A9.0=FMC_A9,13b-sda1
SH.FMC_A9.ConfNb=1
SH.FMC_D0_DA0.0=FMC_D0,sd-16b-d1
SH.FMC_D0_DA0.ConfNb=1
SH.FMC_D10_DA10.0=FMC_D10,sd-16b-d1
SH.FMC_D10_DA10.ConfNb=1
SH.FMC_D11_DA11.0=FMC_D11,sd-16b-d1
SH.FMC_D11_DA11.ConfNb=1
SH.FMC_D12_DA12.0=FMC_D12,sd-16b-d1
SH.FMC_D12_DA12.ConfNb=1
SH.FMC_D13_DA13.0=FMC_D13,sd-16b-d1
SH.FMC_D13_DA13.ConfNb=1
SH.FMC_D14_DA14.0=FMC_D14,sd-16b-d1
SH.FMC_D14_DA14.ConfNb=1
SH.FMC_D15_DA15.0=FMC_D15,sd-16b-d1
SH.FMC_D15_DA15.ConfNb=1
SH.FMC_D1_DA1.0=FMC_D1,sd-16b-d1
SH.FMC_D1_DA1.ConfNb=1
SH.FMC_D2_DA2.0=FMC_D2,sd-16b-d1
SH.FMC_D2_DA2.ConfNb=1
SH.FMC_D3_DA3.0=FMC_D3,sd-16b-d1
SH.FMC_D3_DA3.ConfNb=1
SH.FMC_D4_DA4.0=FMC_D4,sd-16b-d1
SH.FMC_D4_DA4.ConfNb=1
SH.FMC_D5_DA5.0=FMC_D5,sd-16b-d1
SH.FMC_D5_DA5.ConfNb=1
SH.FMC_D6_DA6.0=FMC_D6,sd-16b-d1
SH.FMC_D6_DA6.ConfNb=1
SH.FMC_D7_DA7.0=FMC_D7,sd-16b-d1
SH.FMC_D7_DA7.ConfNb=1
SH.FMC_D8_DA8.0=FMC_D8,sd-16b-d1
SH.FMC_D8_DA8.ConfNb=1
SH.FMC_D9_DA9.0=FMC_D9,sd-16b-d1
SH.FMC_D9_DA9.ConfNb=1
SH.FMC_NBL0.0=FMC_NBL0,Sd2ByteEnable1
SH.FMC_NBL0.ConfNb=1
SH.FMC_NBL1.0=FMC_NBL1,Sd2ByteEnable1
SH.FMC_NBL1.ConfNb=1
SH.FMC_SDCLK.0=FMC_SDCLK,13b-sda1
SH.FMC_SDCLK.ConfNb=1
SH.FMC_SDNCAS.0=FMC_SDNCAS,13b-sda1
SH.FMC_SDNCAS.ConfNb=1
SH.FMC_SDNRAS.0=FMC_SDNRAS,13b-sda1
SH.FMC_SDNRAS.ConfNb=1
SH.FMC_SDNWE.0=FMC_SDNWE,13b-sda1
SH.FMC_SDNWE.ConfNb=1
SH.GPXTI0.0=GPIO_EXTI0
SH.GPXTI0.ConfNb=1
SH.GPXTI13.0=GPIO_EXTI13
SH.GPXTI13.ConfNb=1
SPI5.BaudRatePrescaler=SPI_BAUDRATEPRESCALER_2
SPI5.CalculateBaudRate=42.0 MBits/s
SPI5.Direction=SPI_DIRECTION_2LINES
SPI5.IPParameters=VirtualType,Mode,Direction,CalculateBaudRate,BaudRatePrescaler
SPI5.Mode=SPI_MODE_MASTER
SPI5.VirtualType=VM_MASTER
TIM7.IPParameters=Prescaler,Period
TIM7.Period=1000-1
TIM7.Prescaler=90-1
USART1.IPParameters=VirtualMode
USART1.VirtualMode=VM_ASYNC
USB_DEVICE.CLASS_NAME_HS=MSC
USB_DEVICE.IPParameters=VirtualMode-MSC_HS,VirtualModeHS,CLASS_NAME_HS,MSC_MEDIA_PACKET-MSC_HS
USB_DEVICE.MSC_MEDIA_PACKET-MSC_HS=4096
USB_DEVICE.VirtualMode-MSC_HS=Msc
USB_DEVICE.VirtualModeHS=Msc_HS
USB_OTG_HS.IPParameters=VirtualMode-Device_Only_FS
USB_OTG_HS.VirtualMode-Device_Only_FS=Device_Only_FS
VP_DMA2D_VS_DMA2D.Mode=DMA2D_Activate
VP_DMA2D_VS_DMA2D.Signal=DMA2D_VS_DMA2D
VP_FATFS_VS_Generic.Mode=User_defined
VP_FATFS_VS_Generic.Signal=FATFS_VS_Generic
VP_FREERTOS_VS_CMSIS_V2.Mode=CMSIS_V2
VP_FREERTOS_VS_CMSIS_V2.Signal=FREERTOS_VS_CMSIS_V2
VP_SYS_VS_tim6.Mode=TIM6
VP_SYS_VS_tim6.Signal=SYS_VS_tim6
VP_TIM7_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM7_VS_ClockSourceINT.Signal=TIM7_VS_ClockSourceINT
VP_USB_DEVICE_VS_USB_DEVICE_MSC_HS.Mode=MSC_HS
VP_USB_DEVICE_VS_USB_DEVICE_MSC_HS.Signal=USB_DEVICE_VS_USB_DEVICE_MSC_HS
board=custom
rtos.0.ip=FREERTOS
